Wireless Packet/Payload

MicroSD ID

Sequence Number (1 bytes)

GPS Time (9 bytes) Time packet was generated.

FPGA Status –Devices on

Battery State – Voltage, Current, Capacity

SD Card State – Last block written

GPS Position

GPS Accuracy

GPS Position Time

IMU Activity Indicator

Audio Activity Indicator

Solar Controller State

Real Time Clock Alarm Time

Last command received and time received

Temperature